**The Effect of Surface Coating of Iron Oxide Nanoparticles on Magnetic Resonance Imaging Relaxivity**

Fatemeh Ahmadpoor1, Atif Masoud2, Neus Feliu3,4, Wolfgang J. Parak4, Seyed Abbas Shojaosadati5\*

1 Department of Materials Engineering, Tarbiat Modares University, Tehran, Iran, f.ahmadpoor@modares.ac.ir

2 Karachi Institute of Radiotherapy and Nuclear Medicine, Karachi, Pakistan, atif\_cancer@hotmail.com

3 Fraunhofer Center for Applied Nanotechnology (CAN), Hamburg, Germany, nfeliu@physnet.uni-hamburg.de

4 Fachbereich Physik and CHyN, Universität Hamburg, 22607 Hamburg, Germany, wolfgang.parak@uni-hamburg.de

5 Biotechnology Group, Faculty of Chemical Engineering, Tarbiat Modares University, Tehran, Iran, shoja\_sa@modares.ac.ir

**\***Correspondence: shoja\_sa@modares.ac.ir

**Supporting Information**



Figure SI-1: X-ray diffraction spectrum of IONPs with dc = 6 nm given as intensity in dependence of the scattering angle 2Θ.



Figure SI-2: Magnetization M in dependence of the applied field H, as recorded for IONPs with dc = 6nm.



Figure SI-3: Fourier-transformed IR spectrum of IONPs with dc = 6 nm showing the transmission T in dependence of the wavenumber.